Configure a DHCP on router one a follows:

1)Excluded address range 10.1.1.1 to 10.1.1.100

2)Pool name = PC

3)Network Gateway = 10.1.110/24

4) Default gateway = Router 1

5) DNS server = router 1

6)Test that PC can ping loop back of router 1

